| TIBURON(GK) >2003 > G 2.0 DOHC > Fuel System > Fuel Delivery System > Accelerator Pedal and Cable>Repair procedures |

REMOVAL
1. | Disconnect the accelerator cable from the accelerator pedal by removing the 2 bolts(A).
2. | After disconnecting the accelerator cable, loosen the bolts(A) of the accelerator arm bracket and remove.
INSTALLATION
1. | When installing the return spring and accelerator pedal, apply multi-purpose grease around each moving point (A) of the accelerator pedal.
2. | Apply sealant to the bolt mounting holes(A), and tighten the accelerator pedal bracket.
Tightening torque Accelerator pedal bracket bolts : 8 ~ 12Nm (80 ~ 120 kg•cm, 5.8 ~ 7.2 lb•ft)
3. | Securely install the resin bushing of the accelerator cable on the end of the accelerator pedal.
4. | Apply multipurpose grease around the cable end (A).
INSPECTION
1. | Check the inner and outer cable for damage.
2. | Check the cable for smooth movement.
3. | Check the accelerator pedal for deformation.
4. | Check the return spring for deterioration.
5. | Check the connection of the bushing to end metal fitting.