| TIBURON(GK) >2003 > G 2.0 DOHC > Body (Interior and Exterior) > Seat & Power Seat > rear seat>Repair procedures |

REMOVAL AND INSTALLATION
1. | Remove the mounting bolts and bracket from the rear seat back.
Tightening torque: 17~26 Nm (170~260 kg•cm, 12.2~18.7 lb•ft)
2. | Remove the mounting bolts from the rear seat cushion.
Tightening torque: 17~26 Nm (170~260 kg•cm, 12.2~18.7 lb•ft)
3. | Installation is the reverse of removal.