| TIBURON(GK) >2003 > G 2.0 DOHC > Engine Mechanical System > Cooling System > Engine Coolant Hose / Pipes>Repair procedures |

INSPECTION
Replace if necessary.
REASSEMBLY
Fit an O - ring in the groove provided at the coolant inlet pipe end, wet the O - ring with coolant and insert the coolant inlet pipe.
• | Do not apply oil or grease to the coolant pipe O - ring.
• | Keep the coolant pipe connections free from sand, dust, etc.
• | Insert the coolant pipe fully into the coolant pump.
• | Do not reuse O - ring. Replace it with a new one.