| TIBURON(GK) >2003 > G 2.0 DOHC > Fuel System > Engine Control System > Throttle Body>Repair procedures |

REMOVAL
The throttle valve must not be removed.
Remove the throttle position sensor.
Except when necessary for replacement, the throttle position sensor must not be removed.
INSPECTION
1. | Check the throttle body for cracks.
2. | Check for restriction in the vacuum port or passage.
3. | Check for interference when moving the accelerator cable.
• | Throttle valve set screw is set by the factory. Please do not adjust this screw.
• | When the idle rpm is out of specification, check the relevant sensors and their input or output value first.