| TIBURON(GK) >2003 > G 2.0 DOHC > Body (Interior and Exterior) > General Information>Specifications |

SPECIFICATIONS
Hood
- | Type
| Rear hinged, front opening type (gaslifter type)
Door
- | Construction
- | Regulator system
- | Locking system
| Front hinged, full door construction Wire drum type Pin-fork system
Tailgate
- | Type
| Inner hinged, gas lifter type
Glass thickness mm(in.)
- | Windshield glass
- | Door glass
- | Quarter fixed glass
- | Tailgate glass
| 5 (0.20) 5 (0.20) 3.2 (0.13) 3.5 (0.14)
Seat belt | 3 point type with E.L.R
E.L.R. : Emergency Locking Retractor
TIGHTENING TORQUE
| Nm | Kg•cm | lb•ft
Door
- | Door hinge to body
- | Door hinge to door
- | Door striker mounting bolt
| 35~42 10~12 17~22 | 350~420 100~120 170~220 | 25~31 7~8 12~16
Tailgate
- | Tailgate hinge to body
- | Tailgate hinge to tailgate
- | Tailgate latch mounting bolt
- | Tailgate striker mounting bolt
| 22~27 7~9 7~11 9~14 | 220~270 70~90 70~110 90~140 | 16~19.5 5~7 5~8 6.5~10
Hood
- | Hood hinge to body
- | Hood hinge to hood
- | Hood latch to body
- | Gas lifter mounting bolt
| 22~27 22~27 7~11 9~14 | 220~270 220~270 70~110 220~270 | 16~19.5 16~19.5 5~8 16~19.5
Seat
- | Front seat to floor, Bolt
- | Rear seat back center bracket, Bolt
- | Rear seat back lower side bracket, Bolt
- | Rear seat cushion mounting, Bolt
| 35~55 17~26 17~26 17~26 | 350~550 170~260 170~260 170~260 | 25~40 12~19 12~19 12~19
Seat belt
- | Front seat belt retractor mounting bolt
- | Front seat belt upper anchor mounting bolt
- | Front seat belt sliding bar mounting bolt
- | Front seat belt height adjuster mounting bolt
- | Rear seat belt retractor mounting bolt
- | Rear seat belt upper anchor mounting bolt
- | Front seat belt buckle mounting bolt
| 40~55 40~55 40~55 40~55 40~55 40~55 40~55 | 400~550 400~550 400~550 400~550 400~550 400~550 400~550 | 29~40 29~40 29~40 29~40 29~40 29~40 29~40
Sunroof
- | Sunroof lid panel mounting, Nut
- | Sunroof assembly mounting, Bolt
| 7~9 7~11 | 70~90 70~110 | 5~6.5 5~8