| TIBURON(GK) >2003 > G 2.0 DOHC > Heating,Ventilation, Air Conditioning > General Information>Specifications |

SPECIFICATIONS
Item | Specification
Heating | Heater Type Capacity | Air mix type 4,500 ± 10% kcal/hr
Air conditioning | Evaporator Cooling capacity | 4,100 ± 10% kcal/hr
Compressor Type Oil capacity Pressure relief valve Voltage | Swash plate (HS-15) 140 ~ 160cc Operating pressure : 35 ~ 42.2kg/cm² D.C 12.8 ± 0.2V
Magnetic clutch Voltage & wattage Torque | D.C 12.8 ± 0.2V, Max. 54W Min. 4.4kg•m
Refrigerant & capacity | R-134a (600 ± 25g)
Triple pressure switch | High pressure ON 32.0 ± 2.0kg/cm² OFF 26.0 ± 2.0kg/cm²
Middle pressure ON 18.0 ± 0.8kg/cm² OFF 14.0 ± 1.2kg/cm²
Low pressure ON 2.3 + 0.25 / -0.29kg/cm² OFF 2.0 ± 0.2kg/cm²
Thermistor | OFF 1.5 ± 0.6°C ON 3.0 ± 0.6°C
Heater control assembly | MANUAL Type, AUTOMATIC Type