| TIBURON(GK) >2003 > G 2.0 DOHC > Engine Mechanical System > Intake And Exhaust System > Intake Manifold>Repair procedures |

REMOVAL
1. | Remove the engine cover.
2. | Remove the intake air hose connected to the throttle body.
3. | Remove the accelerator cable.
4. | Remove the P.C.V. hose and brake booster vacuum hoses.
5. | Disconnect the vacuum hose connections, ISA and TPS connector.
6. | Disconnect the high pressure fuel hose connection after relieving pressure in the fuel rail to prevent fuel from spilling.
7. | Remove the intake manifold.
8. | Remove the intake manifold assembly and gasket.
9. | Disconnect the fuel injector harness connector.
10. | Remove the delivery pipe with the fuel injectors.
Be careful not to drop the injectors when removing the delivery pipe.
INSTALLATION
1. | Replace the intake manifold gasket and install the intake manifold.
Be careful not to drop the injectors when removing the delivery pipe.
2. | Install the delivery pipe with the fuel injectors.
3. | Connect the fuel injector harmess connector.
4. | Install the intake manifold stay.
5. | Connect the high pressure fuel hose connection.
6. | Install the P.C.V hose and brake booster vacuum hose.
7. | Install the intake air hose to the throttle body.
8. | Install the accelorator cable.
9. | Connect the ISA and TPS wire harness connector.
INSPECTION
Check the parts for damage or cracking. AIR HOSE Check for damage or cracking of any part.