| TIBURON(GK) >2003 > G 2.0 DOHC > Emission Control System > General Information>Specifications |

SPECIFICATIONS
Components | Function | Remarks
Crankcase Emission System Positive Crankcase Ventilation (PCV) valve | HC reduction | Variable flow rate type
Evaporative Emission System EVAP Canister EVAP Canister Purge Solenoid Valve | HC reduction | Duty control solenoid valve
Exhaust Emission System MFI system (air-fuel mixtrue control device) Three-way catalytic converter | CO, HC, NOx reduction CO, HC, NOx reduction | Heated oxygen sensor feedback type Monolithic type
MFI : Multiport Fuel Injection EVAP : Evaporative Emission SERVICE STANDARD
Item | Specifications
Evaporative emission canister purge solenoid valve Coil resistance | 26Ω [at 20°C (68°F)]
TIGHTENING TORQUE
Item | Nm | kg•cm | lb•ft
Positive Crankcase Ventilation Valve | 8 ~ 12 | 80 ~ 120 | 6 ~ 8