| TIBURON(GK) >2003 > G 2.0 DOHC > Fuel System > General Information>Specifications |

SPECIFICATIONS
Items | Specifications
Engine Management System (ECM) | Siemens
Fuel tank Capacity Return system Fuel filter F/Pressure regulator Regulator pressure Fuel pump | 55 lit. (14.5 U.S. gal., 12.1 lmp.gal.) Returnless High pressure type (built in F/Pump Assembly) Built in F/Pump Assembly 350 kpa (3.5 kg/cm², 49.8 psi) Electrical, in-tank type
INPUT SENSORS Mass Air Flow (MAF) sensor Output voltage Throttle body Throttle Position Sensor (TPS) Resistance Output voltage at curb idle Knock sensor Intake Air Temperature sensor (IAT Sensor) Resistance Engine Coolant Temperature sensor (ECT Sensor) Resistance Heated Oxygen Sensor (HO2S) Output voltage (V) Vehicle Speed Sensor Camshaft Position Sensor (CMP Sensor) Output voltage (V) Crankshaft Position Sensor (CKP Sensor) Output voltage (V) Differential Pressure Sensor (DPS) | Hot film type 0 ~ 5V Variable resister type 0.7 ~ 3.0 kΩ 0.1 ~ 0.875V Piezoelectric type Thermistor type (built in MAF sensor) 2.0 ~ 3.0 kΩ at 20°C (68°F) Thermistor type 2.27 ~ 2.73kΩ at 20°C (68°F) 0.30 ~ 0.32kΩ at 80°C (176°F) Zirconia sensor (Heated) 0 ~ 1V Wheel speed sensor (Inductive) Hall effect sensor 0 ~ 5V Hall effect sensor 0 ~ 5V Piezo-Resistivity type
OUTPUT ACTUATORS Injector type Number Coil resistance (Ω) EVAP Canister Purge solenoid valve Resistance Idle Speed Control actuator (ISC Actuator) Control frequency (Hz) Canister Close Valve (CCV) | Electromagnetic type 4 14.5 ± 0.7Ω Duty type 26Ω Double coil type 100Hz ON/OFF type
SERVICE STANDARDS
Items | 2.0L
Basic idle rpm Ignition timing (°) - BTDC | 700 ± 100 (N,A/C OFF) 9° ± 5°
SEALANTS
Engine coolant temperature sensor assembly | LOCTITE 962T or equivalent
TIGHTENING TORQUES
Items | Nm | Kg•cm | lb•ft
Delivery pipe installation bolts Heated oxygen sensor Crankshaft position sensor installation bolts Knock sensor installation bolt Engine coolant temperature sensor Throttle position sensor installation bolts Throttle body to surge tank bolts | 19 ~ 28 50 ~ 60 4 ~ 6 17 ~ 27 15 ~ 20 1.5 ~ 2.5 19 ~ 28 | 190 ~ 280 500 ~ 600 40 ~ 60 170 ~ 270 150 ~ 200 15 ~ 25 180 ~ 280 | 14 ~ 20.7 37 ~ 44 3 ~ 4.4 12.5 ~ 20 11 ~ 15 1.1 ~ 1.8 14 ~ 20.7