| TIBURON(GK) >2003 > G 2.0 DOHC > Body Electrical System > Keyless Entry And > Transmitter>Repair procedures |

INSPECTION
1. | Check that the red light flickers when the door lock button or unlock button is pressed on the transmitter.
2. | Remove the battery and check voltage if the red light doesn't flicker.
Standard voltage : 3V
1. | Replace the battery if voltage is below 3V and replace the remote control switch if it is inoperable after replacing the battery.
Battery : Lithium CR2032 (3V, 220mA/h)
TRANSMITTER CODE SAVING METHOD
1. | To store transmitter code, first connect the hi-scan (pro) to the Data Link Connector (DLC) in driver side crash pad lower panel.
2. | Turn the power on hi-scan (pro) with the ignition switch ON.
3. | Select the vehicle model on hi-scan (pro).
4. | After selecting "CODE SAVING" menu then button "ENTER" key.
5. | Proceed as follow steps and then code saving is completed.
(1) | Press [ENTER] key, if you are ready.
(2) | Press the transmitter [LOCK] button above 1 second.
(3) | If you save transmitter one more, press other transmitter [LOCK] button above 1 second.
(4) | Turn the hi-scan (pro) off, and check the keyless entry system.
INSPECTION
1. | Check that the red light flickers when the door lock button or unlock button is pressed on the transmitter.
2. | Remove the battery and check voltage if the red light doesn't flicker.
Standard voltage : 3V
3. | Replace the battery if voltage is below 3V and replace the remote control switch if it is inoperable after replacing the battery.
Battery : Lithium CR2032 (3V, 220mA/h)
PROGRAMMING TRANSMITTER CODE
1. | To program the transmitter code, first connect the hi-scan (pro) to the Data Link Connector (DLC) in drive side crash pad lower panel.
2. | Turn the power on hi-scan (pro) with the ignition switch ON.
3. | Select the vehicle model on hi-scan (pro).
4. | After selecting "CODE SAVING" menu then button "ENTER" key.
5. | Proceed as follow steps and then code saving is completed.
(1) | Press [ENGER] key, if you are ready.
(2) | Press the transmitter [LOCK] button above 1 second.
(3) | If you save transmitter one more, press other transmitter [LOCK] button above 1 second.
(4) | Turn the hi-scan (pro) off, and check the keyless entry system.