| TIBURON(GK) >2003 > G 2.0 DOHC > Body (Interior and Exterior) > Bumper > rear bumper>Repair procedures |

REMOVAL AND INSTALLATION
1. | Loosen the luggage side cover mounting screws and remove the luggage side cover.
2. | Remove the rear combination lampl. Disconnect the combination lamp connector.
3. | Loosen the rear bumper cover mounting screw from the rear wheel house.
4. | Loosen the rear bumper cover mounting screw from the rear wheel house.
5. | Loosen the rear bumper upper part mounting screws.
6. | Loosen the rear bumper lower part mounting screws.
When installing, align the protrusion of the bumper cover with the groove of the panel.
7. | Disconnect the licence lamp connector from the rear bumper cover and remove the rear bumper beam assembly.
Tightening torque: 25~30 Nm (250~300 kg•cm, 18.0~21.6 lb•ft)
8. | Installation is the reverse of removal.