| TIBURON(GK) >2003 > G 2.7 DOHC > Engine Mechanical System > Cylinder Block > Engine Mounts>Repair procedures |

REMOVAL
Attach a chain or cable to the engine hooks and lift enough so that there is no pressure on the motor mounts. Engine Mounting
1. | Remove the engine mounting insulator bolts.
2. | Remove the engine mounting bracket from the engine.
Transaxle Mounting
1. | Remove the transaxle mounting insulator bolts.
2. | Remove the tranaxle mounting bracket from the transaxle.
Front Roll Stopper Remove the front roll stopper bracket from the sub-frame. Rear Roll Stopper
1. | Remove the bolt from the rear roll stopper.
2. | Remove the rear roll stopper from the subframe.