| TIBURON(GK) >2003 > G 2.7 DOHC > Body (Interior and Exterior) > Bumper > front bumper>Repair procedures |

REMOVAL AND INSTALLATION
1. | Remove the front bumper upper cover.
2. | Loosen the head lamp mounting bolts, disconnect the connector, and remove the head lamp assembly.
3. | Disconnect the fog lamp connectors.
4. | Remove the front bumper upper mounting bolt and screws.
Tightening torque: 4~6 Nm (40~60 kg•cm, 2.9~4.4 lb•ft)
5. | Remove the mounting screws in the corner of front bumper.
Tightening torque: 4~6 Nm (40~60 kg•cm, 2.9~4.4 lb•ft)
6. | Loosen the front bumper lower mounting screws and remove the front bumper cover.
7. | Remove the front bumper upper mesh.
8. | After loosening the front bumper beam stay mounting bolts and nuts and remove the front bumper beam stay.
9. | Installation is the reverse of removal.