| TIBURON(GK) >2003 > G 2.7 DOHC > Body Electrical System > Audio > Speakers>Repair procedures |

REMOVAL
FRONT SPEAKER
1. | Remove the front door trim panel and remove the front speaker.
2. | Installation is the reverse of removal.
REAR SPEAKER
1. | Remove the quarter trim and remove the rear speaker.
2. | Installation is the reverse of removal.
AMP
1. | Remove the quarter trim.
2. | Remove the amp from the left side quarter panel.
INSPECTION
1. | Check the speaker with an ohmmeter. If an ohmmeter indicates the correct impedance of the speaker when checking between the speaker (+)and speaker (-) of the same channel, the speaker is ok.
2. | If a clicking sound is emitted from the speaker when the ohmmeter is connected to the speaker terminals, the speaker is ok.