| TIBURON(GK) >2003 > G 2.7 DOHC > Suspension System > Rear Suspension System > Rear Suspension Arm>Repair procedures |

REMOVAL
1. | Remove the wheel and tire.
2. | Remove the stabilizer link.
3. | After loosening the rear trailing arm mounting bolts, remove the trailing arm.
4. | Remove the rear suspension arm mounting bolt from the rear axle carrier.
5. | After supporting the center of the rear crossmember assembly with a jack, remove the rear crossmember mounting bolts to the body.
6. | Remove the rear crossmember and suspension arm.
INSTALLATION
1. | Installation is in the reverse order of removal.
2. | Tighten the components below to the specified torque as follows.
Items | Torque Nm (kgf•cm, lbf•ft)
* Trailing arm mounting | 100~120 (1000~1200, 74~88)
Trailing arm bracket mounting | 40~50 (400~500, 29~37)
Stabilizer bar bracket mounting | 17~26 (170~260, 13~19)
Stabilizer link nut | 34~45 (340~450, 25~33)
*Front/Rear suspension arm mounting | 160~180 (1600~1800, 118~133)
Rear crossmember mounting | 100~120 (1000~1200, 74~88)
INSPECTION
1. | Check the rubber parts for damage or deterioration.
2. | Check the trailing arm and suspension arm for bent or deterioration.
3. | Check the bolts for damage or rust.