| TIBURON(GK) >2003 > G 2.7 DOHC > Engine Mechanical System > Intake And Exhaust System > Muffler>Repair procedures |

REMOVAL
Main Muffler
Before removing or inspecting the exhaust system, ensure that the exhaust system is cool.
1. | Disconnect the main muffler from the center exhaust pipe.
2. | Remove the rubber hangers and the main muffler.
Front Exhaust Pipe (Including catalytic converter)
1. | Remove the front exhaust pipe from the center exhaust pipe.
2. | Remove the front exhaust pipe bolt and the exhaust manifold pipe mounting nuts.
3. | Remove the front exhaust pipe.
INSTALLATION
1. | Temporarily install the front exhaust pipe, the catalytic converter assembly, the center exhaust pipe and the main muffler, in this order.
2. | Install the rubber hangers so that they hang equally left and right.
3. | Tighten the parts securely and then confirm that there is no interference with any components.
INSPECTION
1. | Check the mufflers and pipes for leaks, corrosion and damage.
2. | Check the rubber hangers for deterioration and cracks.