| TIBURON(GK) >2003 > G 2.7 DOHC > Clutch System > Clutch System > Clutch Master Cylinder>Repair procedures |

DISASSEMBLY
1. | Remove the reservoir band, reservoir tank and reservoir cap.
2. | Remove the piston stop ring.
3. | Pull out the push rod and piston assembly.
Be careful not to damage the master cylinder body and piston assembly.
INSPECTION
1. | Check the inside of the cylinder body for rust, pitting or scoring.
2. | Check the piston cup for wear or distortion.
3. | Check the piston for rust, pitting or scoring.
4. | Check the clutch tube line for obstructions.
5. | Measure the clutch master cylinder inside diameter with a cylinder gauge and the piston outside diameter with a micrometer.
Measure the inside diameter of the clutch master cylinder in three places (bottom, middle, and top), in perpendicular directions.
6. | If the clutch master cylinder-to-piston clearance exceeds the limit, replace the master cylinder and/or piston assembly.
0.15 mm (0.006 in.)
REASSEMBLY
1. | Apply the specified fluid to the inner surface of the cylinder body and to the outside of the piston assembly.
BRAKE FLUID DOT 3 or DOT 4
2. | Install the piston assembly.
3. | Install the piston stop ring.
4. | Install the push rod assembly.
5. | Install the reservoir band, reservoir tank and reservoir cap.