| TIBURON(GK) >2003 > G 2.7 DOHC > Brake System > ABS(Anti-Lock Brake System) > Front Wheel Speed Sensor>Repair procedures |

REMOVAL
FRONT WHEEL SPEED SENSOR
1. | Remove the front wheel speed sensor mounting bolt.
2. | Remove the front wheel speed sensor after disconnecting the wheel speed sensor connector.
REAR WHEEL SPEED SENSOR
1. | Remove the rear wheel speed sensor mounting bolt.
2. | Remove the luggage trim and disconnect the wire connector from the rear wheel speed sensor.
INSPECTION
1. | Connect an ohmmeter between the wheel speed sensor terminals and measure the resistance.
Service standard Front, Rear: 1,385 ± 110Ω
2. | Connect a voltmeter between the wheel speed sensor terminals and measure the voltage by turning the wheel.
Set the voltmeter to measure AC voltage. Service standard : AC voltage detected.