| TIBURON(GK) >2004 > G 2.0 DOHC > Engine Mechanical System > Cylinder Block > Engine Mounts>Repair procedures |

REMOVAL
1. | Attach an engine hoist to the engine hooks, and raise the engine just enough so that there is no pressure on the insulators.
ENGINE MOUNTING
1. | Remove the engine mounting insulator bolts.
2. | Remove the engine mounting bracket from the engine.
TRANSMISSION MOUNTING
1. | For vehicles with a 5-speed manual transmission, remove the select control valve.
2. | Remove the transmission mounting bolt.
3. | Detach the cap from inside the right fender shield. Remove the transmission mounting bolts.
4. | Remove the transmission bracket.
FRONT ROLL STOPPER
1. | Remove the front roll stopper bracket from the subframe.
REAR ROLL STOPPER
1. | Remove the rear roll stopper from the subframe.