| TIBURON(GK) >2004 > G 2.0 DOHC > Engine Mechanical System > Intake And Exhaust System > Air Cleaner>Repair procedures |

REMOVAL
1. | Remove the air duct connected to the air cleaner.
2. | Disconnect the intake air temperature sensor harness.
3. | Remove the air intake hose at the air cleaner side.
4. | Remove the air cleaner cover and filter.
5. | Remove the air cleaner mounting bolts and remove the air cleaner.
INSTALLATION
Install the air cleaner assembly following the reverse order of removal.
INSPECTION
1. | Check the air cleaner body, cover, or filter for distortion, corrosion or damage.
2. | Check the air duct for damage.
3. | Check the resonator for distortion or damage.
4. | Check the air cleaner filter for restriction, contamination or damage. If the filter is slightly restricted, remove the dust and other contaminants by blowing compressed air from the upper side through the filter.
5. | Check the air cleaner housing for restrictions, contamination or damage.