| TIBURON(GK) >2004 > G 2.0 DOHC > Steering System > General Information>Specifications |

SPECIFICATIONS
Item | Specification
Steering gear type Rack stroke Power steering pump type Oil pump displacement | Rack and pinion 132mm Vane type 9.6 cm³/rev.MAX. (0.59 in³/rev.MAX.)
SERVICE STANDARD
Item | Specification
Steering wheel free play Steering angle Inner wheel Outer wheel Stationary steering effort Belt deflection New belt Used belt Oil pump relief pressure Total pinion preload Tie rod swing resistance Tie rod end ball joint starting torque | 0~30 mm (0~1.1 in.) 34°76´ ± 2° 30°19´ 29N (3.0kg, 6.5lbs) 8.8~11.0 12.5~14.3 8.3~8.8 MPa (85~90 kg/cm², 1209~1280 psi 0.6~1.3 Nm (6~13 kg•cm, 5.2~11.3 lb•in.) 2~5 Nm (20~50 kg•cm, 1.4~3.6 lb•ft) 0.5~2.5 Nm (5~25 kg•cm, 0.36~1.78 lb•ft)
TIGHTENING TORQUE
Item | Nm | kg•cm | lb•ft
Power steering column and shaft Steering column and shaft assembly mounting bolt Power steering wheel lock nut Pinion gear and joint assembly Steering column shaft and universal joint assembly Dust cover mounting bolt | 13 ~ 18 35 ~ 45 15 ~ 20 18 ~ 20 17 ~ 26 | 130 ~ 80 350 ~ 450 150 ~ 200 180 ~ 200 170 ~ 260 | 9.6 ~ 13.3 25.8 ~ 33.2 11 ~ 15 13.3 ~ 15 125. ~ 19.2
Power steering gear box Gear box mounting bolt Tie rod end lock nut Tie rod end ball joint and knuckle arm mounting nut Feed tube to gear box Gear box to valve body Yoke plug lock nut | 60 ~ 80 50 ~ 55 24 ~ 34 10 ~ 16 20 ~ 30 50 ~ 70 | 600 ~ 800 500 ~ 550 240 ~ 340 100 ~ 160 200 ~ 300 500 ~ 700 | 44 ~ 59 37 ~ 40.6 17.7 ~ 25 7.4 ~ 11.8 15 ~ 22 37 ~ 52
Power steering oil pump Pressure hose to oil pump Oil pump adjusting bolt Oil pump mounting bolt Oil pump bracket mounting bolt | 55 ~ 65 35 ~ 50 35 ~ 50 35 ~ 50 | 550 ~ 650 350 ~ 500 350 ~ 500 350 ~ 500 | 40.6 ~ 47.9 25.8 ~ 37 25.8 ~ 37 25.8 ~ 37
Power steering hose Power steering reservoir mounting bolt Power steering hose mounting bolt Power steering tube mounting bolt | 4 ~ 6 4 ~ 6 4 ~ 6 | 40 ~ 60 40 ~ 60 40 ~ 60 | 3.0 ~ 4.4 3.0 ~ 4.4 3.0 ~ 4.4
LUBRICANTS
| Recommended lubricant | Quantity
Horn contact ring of steering wheel | CENTOPLX278 (KLUBER KOREA) | 1.5g
Bearing of steering shaft | ALVANIA #2 or #3 (KEUK DONG SHELL, KOREA) | As required
Ball joint of tie rod end | SHOWA SUNLIGHT MB-2 or equivalent | 1.5g
Steering gear housing | ONE-LUBER RP GREASE (KYODOYUSHI, JAPAN) | As required
Inner ball joint of gear box | LONG TIME PD2 (OPTIMOL, GERMAN) | As required
Contact area of gear box bellows & tie rod | SILICON GREASE (SPEC NO : MS511-41) | As required
Power steering fluid | PSF-3 | 0.75 ~ 0.8 liter (0.79 ~ 0.84 qts.)