| TIBURON(GK) >2004 > G 2.0 DOHC > Body (Interior and Exterior) > Seat Belt > rear seat belt>Repair procedures |

REMOVAL AND INSTALLATION
1. | Remove the mounting bolts from the rear seat cushion.
2. | Remove the mounting bolts from the rear seat back.
3. | Remove the rear seat back lower side mounting bracket.
Tightening torque: 40~55 Nm (400~500 kg•cm, 25~40 lb•ft)
4. | Loosen the rear seat belt upper, lover mounting bolts, and remove the rear seat belt.
5. | Installation is the reverse of removal.
REAR SEAT BELT BUCKLE
1. | Remove the mounting bolts from the rear seat cushion.
Tightening torque: 17~26 Nm (170~260 kg•cm, 12~19 lb•ft)
2. | Remove the rear seat belt buckle.
3. | Installation is the reverse of removal.