| TIBURON(GK) >2004 > G 2.0 DOHC > Body Electrical System > Windshield Wiper/Washer > Front Washer Motor>Repair procedures |

INSPECTION
1. | With the washer motor connected to the reservoir tank, fill the reservoir tank with water.
2. | Connect positive (+) and negative (-) battery cables to terminals 2 and 1 respectively to see that the washer motor runs and water sprays fromthe front nozzles.
3. | Check that the motor operates normally.