| TIBURON(GK) >2004 > G 2.0 DOHC > Body Electrical System > Multifunction switch > Multi Function Switch>Repair procedures |

REMOVAL
• | Never attempt to disassemble or repair the air bag module or clock spring. If faulty, replace it.
• | Do not drop the air bag module or clock spring or allow contact with water, grease or oil. Replace if a dent, crack, deformation or rust is detected.
• | The air bag module should be stored on a flat surface and placed so that the pad surface is facing upward. Do not place anything on top of it.
• | Do not expose the air bag module to temperatures over 93°C(200°F).
• | After deployment of an air bag, replace the clock spring with a new one.
• | Wear gloves and safety glasses when handing an air bag that has been deployed.
• | An undeployed air bag module should only be disposed of in accordance with the procedures mentioned in the restraints section.
• | When you disconnect the air bag module-clock spring connector, take care not to apply excessive force.
• | The removed air bag module should be stored in a clean, dry place.
• | Prior to installing the clock spring, align the mating mark and "NEUTRAL" position indicator of the clock spring, and after turning the front wheels to the straight-ahead position, install the clock spring to the column switch. If the mating mark of the clock spring is not properly aligned, the steering wheel may not completely rotate during a turn, or the flat cable within the clock spring may be broken obstructing normal operation of the SRS and possibly leading to serious injury to the vehicle's driver. To inspect the clock spring,refer to the restraints section.
1. | Remove the air bag module.
2. | Remove the steering wheel.
3. | Remove the steering column upper shroud and steering column lower shroud.
4. | Remove the 3 screws holding the multi function switch and disconnect the connectors. Remove the multi function switch assembly.
5. | Installation is the reverse of removal.
INSPECTION
LIGHTING SWITCH [M01-2]
DIMMER AND PASSING SWITCH [M01-2]
TURN SIGNAL AND LANE CHANGE SWITCH [M01-2]
WIPER AND INTERMITTENT VOLUME SWITCH [M01-1]
WASHER SWITCH [M01-1]
REAR WIPER AND WASHER SWITCH [M01-1]