| TIBURON(GK) >2004 > G 2.0 DOHC > Driveshaft and axle > Driveshaft Assembly > Center Bearing And Inner Shaft>Repair procedures |

DISASSEMBLY
1. | Using the special tool (09517-43001), disassemble the center bearing bracket from the inner shaft.
2. | Using the special tools (09216-21100, 09495-33100), press out the center bearing from the outside to the inside direction of the center bearingbracket as shown in the illustration.
INSPECTION
1. | Check the inner shaft for damage, bending or rust.
2. | Check the inner shaft splines for wear or damage.
3. | Check the center bearing for scoring, discoloration and roughness of the roller journals moving surfaces.
REASSEMBLY
1. | Apply multipurpose grease to the center bearing and inside the center bearing bracket.
2. | Using the special tool (09495-33100), press the center bearing into the center bearing bracket.
3. | Apply multipurpose grease to the rear surface of all dust seals.
Recommended grease : Sunlight No.2 Inner dust seal : 7~10 gr. Outer dust seal : 4~6 gr.
4. | Install the inner shaft into the center bearing bracket.