| TIBURON(GK) >2004 > G 2.0 DOHC > Body (Interior and Exterior) > Exterior > front door>Repair procedures |

REMOVAL AND INSTALLATION
1. | Remove the grip handle using a remover.
2. | Remove the inside handle housing.
3. | Remove the tweeter speaker using a remover.
4. | Remove the mounting screws and remove the door trim panel. Disconnect the wire connectors.
5. | Remove the door grip handle mounting bracket, speaker and door trim seal.
6. | Remove the door tooling hole cover.
7. | Remove the door glass stopper catch.
Tightening torque: 4~6 Nm (40~60 kg•cm, 3~5 lb•ft)
8. | Remove the door delta chassis.
9. | Remove the glass stopper bolts, remove the window glass.
10. | Remove the door side weather strip.
11. | Loosen the mounting nuts and remove the regulator assembly.
Tightening torque: 9~14 Nm (90~140 kg•cm, 6.5~10 lb•ft)
12. | Disconnect the cable, after loosening the inner handle mounting screw, push the inner handle toward the direction shown in the illustrationand remove it.
13. | Remove the door outside belt.
Install the door outside belt to the inside of groove of the door panel.
14. | Remove the door outside handle and key cylinder.
15. | Remove the door latch assembly mounting screws and remove the door latch assembly.
Tightening torque: 17~22 Nm (170~220 kg•cm, 12~16 lb•ft)
16. | Remove the door checker.
17. | Installation is the reverse of removal. When installing the door vapor barrier, butyl tape should not be placed so it blocks the door trim fastener holes.
ADJUSTMENT
DOOR POSITION
Attach protective tape to the fender edges where the hinge is installed.
DOOR STRIKER
1. | Draw a line around the striker plate for reference.
2. | Loosen the striker screws and move the striker IN or OUT to make the latch fit tighter or looser. Move the striker UP or DOWN to align it withthe latch opening. Then lightly tighten the screws and recheck.
Hold the outside handle out and push the door aginst the body to ensure the striker allows a flush fit.