| TIBURON(GK) >2004 > G 2.0 DOHC > Body (Interior and Exterior) > Sun Roof > sun roof switch>Repair procedures |

INSPECTION
1. | Disconnect the negative (-) battery terminal.
2. | Detach the lamp lens then remove the mounting screws (2EA) and open the overhead console case cover then remove the mounting screws (2EA).
1. | After disconnecting the roof wiring and sunroof wiring connector then remove the overhead console lamp assembly from the headliner.
2. | Using an ohmmeter, check for continuity between the terminals. If the continuity is not as specified, replace the sun roof switch.
1. | Verify power and ground continuity between the M95 and M96 terminals.