| TIBURON(GK) >2004 > G 2.0 DOHC > Engine Mechanical System > Intake And Exhaust System > Muffler>Repair procedures |

REMOVAL
MAIN MUFFLER
Before removing or inspecting the exhaust system, ensure that the exhaust system is cool.
1. | Disconnect the main muffler from the center muffler.
2. | Remove the rubber hangers and remove the main muffler.
CENTER MUFFLER
1. | Remove the center muffler assembly from the main muffler and front exhaust pipe.
2. | Remove the rubber hanger, then remove the center muffler.
FRONT EXHAUST PIPE
1. | Remove the front exhaust pipe clamp bolts. and remove the front exhaust pipe nuts from the catalytic converter.
2. | Remove the front exhaust pipe and center muffler bolt.
INSTALLATION
1. | Temporarily install the front exhaust pipe, the center exhaust pipe, and the main muffler, in that order.
2. | Tighten the parts securely. Make sure there is no interference with any body components.