| TIBURON(GK) >2004 > G 2.0 DOHC > Brake System > Brake System > Rear Disc Brake>General Information |

General information
Frequent inhalation of brake pad dust, regardless of material composition, could be hazardous to your health.
• | Avoid breathing dust particles.
• | Never use an air hose or brush to clean brake assemblies.
Remove, disassemble, inspect, reassemble, and install the caliper and note these items:
• | Do not spill brake fluid on the vehicle; it may damage the paint; If brake fluid gets on the paint, wash it off immediately with water.
• | Clean all parts in brake fluid and air dry; blow out all passages with compressed air.
• | Before reassembling, check that all parts are free of dirt and other foreign particles.
• | Replace parts with new ones as specified in the illustration.
• | Make sure no dirt or other foreign matter gets into the brake fluid.
• | Make sure no grease or oil gets on the brake discs or pads.
• | When reusing pads, always reinstall them in their original positions to prevent loss of braking efficiency.
• | Do not reuse drained brake fluid.
• | Always use Genuine DOT 3 or DOT 4 brake fluid. Non Genuine DOT 3 or DOT 4 brake fluid cause corrosion and shorten the life of the system.
• | Coat the piston, piston seal groove, and caliper bore with clean brake fluid.
• | Replace all rubber parts with new ones.
• | After installing the caliper, check the brake hose and line for leaks, interference, interference, and twisting.