| TIBURON(GK) >2004 > G 2.7 DOHC > Body (Interior and Exterior) > Exterior > mirror>Repair procedures |

REMOVAL AND INSTALLATION
OUTSIDE REARVIEW MIRROR
1. | Remove the outside rearview mirror cover.
2. | Loosen the mounting bolts, disconnet the connector and then remove the outside rearview mirror.
Tightening torque: 7~11 Nm (70~110 kg•cm, 5~8 lb•ft)
3. | Installation is the reverse of removal.
INSIDE REARVIEW MIRROR
1. | Remove the rearview mirror.
2. | Installation is the reverse of removal.
DISASSEMBLY
Wear gloves to remove and install the mirror holder.
1. | Insert a flat tip screwdriver between the outside rear view mirror holder and mirror assembly.
When prying with a flat tip screwdriver, wrap it with a shop towel to prevent damage.
2. | Remove the outside rear view mirror actuator from outside rear view mirror housing.
3. | Installation is the reverse of removal.