| TIBURON(GK) >2004 > G 2.7 DOHC > Restraint > Supplemental Restraint System Control Module (SRnodeM)>Repair procedures |

REMOVAL
1. | Disconnect the battery negative cable, and wait at least 30seconds before begining work.
2. | Disconnect the airbag connectors.
3. | Remove the center console. (see BD group).
4. | Disconnect the connector from the SRS unit.
5. | Remove the three bolts from the SRS unit, than pull out the SRS unit from the bracket.