| TIBURON(GK) >2004 > G 2.7 DOHC > Restraint > Airbag Module > Passenger Airbag (PAB) Module>Repair procedures |

REMOVAL
1. | Never attempt to disassemble or repair the airbag module.
2. | Do not drop the airbag module or allow contact with water, grease or oil. Replace it if a dent, crack, deformation or rust are detected.
3. | The airbag module should be stored on a flat surface and placed so that the pad surface is facing upward. Do not place anything on top of it.
4. | Do not expose the airbag module to temperature over 93°C (200°F)
5. | An undeployed airbag module should only be disposed in accordance with the procedures.
6. | Never attempt to measure the circuit resistance of the airbag module (squib) even if you are using the specified tester. If the circuit resistance is measured with a tester, accidental airbag deployment will result in serious personal injury.
7. | Whenever the PAB is deployed it should be replaced with a new one assembled with an extension wire. The squib is melt down if the PAB is deployed making the extension wire useless.
1. | Disconnect the battery negative (-) terminal cable.
Wait at least 30 seconds.
2. | Remove the glove box.
3. | Disconnect the PAB module connector.
4. | Remove the crash pad assembly and then undo the PAB module. (Refer to the BD section)
5. | The skin of the passenger airbag module is integrated with the crash pad, therefore, the crash pad must be replaced if the PAB deploys.