| TIBURON(GK) >2004 > G 2.7 DOHC > Manual Transaxle System > General Information>Troubleshooting (M5GF1) |

TROUBLESHOOTING (M/T)
Symptom | Probable cause | Remedy
Vibration, noise | Loose or damaged transaxle and engine mounts | Tighten or replace mounts
Inadequate shaft end play | Correct end play
Worn or damaged gears | Replace gears
Inadequate grade of oil | Replace with specified oil
Low oil level | Replenish
Inadequate engine idle speed | Adjust idle speed
Oil leakage | Broken or damaged, oil seal or O-ring | Replace oil seal or O-ring
Hard shift | Faulty control cable | Replace control cable
Poor contact or wear of synchronizer ring and gear cone | Correct or replace
Weakened synchronizer spring | Replace synchronizer spring
Inadequate grade of oil | Replace with specified oil
Jumps out of gear | Worn gear shift fork or broken poppet spring | Replace shift fork or poppet spring
Synchronizer hub-to-sleeve spline clearance too large | Replace synchronizer hub and sleeve