| TIBURON(GK) >2004 > G 2.7 DOHC > Restraint > Seat Belt Pretensioner > Seat Belt Retractor Pretensioner (BPT)>Repair procedures |

REMOVAL
1. | Disconnect the battery negative (-) terminal.
Wait at least 30 seconds.
2. | Remove the door scuff trim.
3. | Remove the quarter trim after removing seat belt lower anchor bolt.
4. | Remove the upper anchor plate cover and upper anchor plate.
5. | Remove the lower anchor plate and front seat belt.
1. | Never attempt to disassemble or repair the BPT.
2. | Do not drop the BPT or allow contact with water, grease, oil. Replace it if a dent, crack, deformation or rust are detected.
3. | Do not place anything on the BPT.
4. | Do not expose the BPT to temperature over 93°C(200°F).
5. | BPT functions one time only. Be sure to replace the BPT after it is deployed.
6. | Be sure to wear gloves and safety goggles when handling the deployed BPT.