| TIBURON(GK) >2004 > G 2.7 DOHC > Driveshaft and axle > General Information>Special Service Tools |

SPECIAL TOOLS
Tool (Number and Name) | Illustration | Use
09216-21100 Mounting bushing remover and installer |  | Removal of the center bearing (Use with 09495-33100)
09495-33000 Puller |  | Removal of wheel bearing inner race from the hub.
09495-33100 Center bearing remover and installer |  |
1. | Removal of wheel bearing from the knuckle. (Use with 09517-29000)
2. | Installation of hub to the knuckle.
3. | Removal of the center bearing (Use with 09216-21100)
09517-21500 Front hub remover and installer |  |
1. | Removal of front hub from the knuckle. (Use with 09517-29000)
2. | Measurement of front wheel bearing pre-load. (Use with 09532-11600)
09517-29000 Knuckle arm bridge |  |
1. | Removal of wheel bearing outer race from the knuckle. (Use with 09495-33100)
09517-43001 Bearing puller |  | Removal of the center bearing bracket
09532-11600 Preload socket |  | Measurement of front wheel bearing pre-load. (Use with 09517-21500)
09532-11500 Pinion bearing outer race |  | Installation of wheel bearing to the knuckle.
09568-34000 Ball joint puller |  | Separation of front lower arm and tie rod end ball joint.