| TIBURON(GK) >2004 > G 2.7 DOHC > Engine Mechanical System > Intake And Exhaust System > Exhaust Manifold>Repair procedures |

REMOVAL
1. | Remove the heat protector.
2. | Remove the exhaust manifold.
3. | Remove the exhaust manifold gasket.
INSTALLATION
1. | Install the exhaust manifold with gasket.
Tightening torque Exhaust manifold : 30 ~ 35Nm (300 ~ 350kg.cm, 22 ~ 26lb.ft)
Do not re - use an exhaust manifold gasket.
2. | Install the heat protector.
INSPECTION
1. | Check for damage or cracks.
2. | Using a straight edge and feeler gauge, check for distortion on the cylinder head matching surface.
Standard value : 0.15 mm (0.006 in.) or less Service limit : 0.3 mm (0.012 in.) or less
3. | Check the exhaust manifold for damage and cracks.