| TIBURON(GK) >2004 > G 2.7 DOHC > Body Electrical System > Auto Lighting Control System>Description and Operation |

DESCRIPTION
The auto light control system operates by using the auto light switch and the auto light sensor detect the illumination then turns the head lamp and tail lamp on or off automatically in accordance with the detection illumination. SPECIFICATIONS
Items | Specifications
Rated voltage | DC 5V
Operating current | Max. 1mA
Detection illumination | Tail lamp | ON : 23.1 ± 3.4 (Lux), 1.77 ± 0.08 (V) OFF : 48.0 ± 3.4 (Lux), 3.47 ± 0.10 (V)
Head lamp | ON : 6.2 ± 1.4 (Lux), 0.63 ± 0.06 (V) OFF : 12.0 ± 1.4 (Lux), 1.02 ± 0.06 (V)