| TIBURON(GK) >2005 > G 2.0 DOHC > Body (Interior and Exterior) > Exterior > fender>Repair procedures |

REMOVAL AND INSTALLATION
FENDER
1. | Remove the front mud guard and wheel guard.
2. | Remove the 3 bolts holding the head lamp and disconnect the wire connector. Remove the head lamp assembly.
3. | Remove the front bumper. (refer to front bumper group)
4. | Remove the fender mounting bolts and remove the fender panel assembly.
Use care to avoid damaging the paint.
5. | Installation is the reverse of the removal.
In order to prevent the fender mounting bolt area from forming rust, apply tape sealer between the fender and the bodypanel.
FENDER GARNISH
1. | Remove the wheel guard.
2. | Loosen the fender garnish mounting screws and then remove the fender garnish.
3. | Installation is the reverse of the removal.
1. | When installing garnish, be careful not to deform the fender panel.
2. | Engage the clip part on the garnish into the fender panel securely until it makes "click" sound.