| TIBURON(GK) >2005 > G 2.0 DOHC > Fuel System > Fuel Delivery System > Fuel Tank>Repair procedures |

REMOVAL
1. | Remove the rear seat cushion (Refer to "BD" group in this SHOP MANUAL).
2. | Open the service cover (A) under the rear seat cushion.
3. | Release the internal pressure of the fuel lines and hoses as following:
A. | Disconnect the fuel pump assembly harness connector (A).
B. | Start the engine and wait until fuel in fuel line is exhausted. After the engine stalls, turn the ignition switch to OFF position.
C. | Disconnect the negative (-) terminal from the battery.
4. | Disconnect the fuel feed line (B).
Cover the hose connection with a shop towel to prevent splashing of fuel caused by residual pressure in the fuel line
5. | Lift the vehicle.
6. | Disconnect the hoses connected to the fuel tank.
7. | Remove the muffler (A) (Refer to "EM" group in this SHOP MANUAL).
8. | Remove the fuel tank band (B) and remove the fuel tank (C).