| TIBURON(GK) >2005 > G 2.0 DOHC > Body (Interior and Exterior) > Bumper > front bumper>Repair procedures |

REPLACEMENT
FRONT BUMPER COVER REPLACEMENT
1. | Remove the front bumper cover (A).
2. | After loosening the mounting bolt, remove the headlamp (A).
3. | Disconnect the fog lamp connector (A).
4. | Remove the front bumper cover (A).
5. | Installation is the reverse of removal.
FOG LAMP REPLACEMENT
1. | Remove the front bumper cover (See page BD-53).
2. | After loosening the mounting screw, remove the fog lamp (A).
3. | Installation is the reverse of removal.
FRONT BUMPER RAIL REPLACEMENT
1. | Remove the front bumper cover (See page BD-53).
2. | Loosening the front bumper rail mounting bolt, nut.
3. | Remove the front bumper rail (A).
4. | Installation is the reverse of removal.