| TIBURON(GK) >2005 > G 2.0 DOHC > Restraint > Supplemental Restraint System Control Module (SRnodeM)>Troubleshooting |

Hi-Scan check
1. | Turn the ignition switch off.
2. | Connect the Hi-Scan Pro connector to the datalink connector located under the crash pad.
3. | Connect the Hi-Scan Pro power cable.
4. | Turn the ignition switch on and power on the Hi-Scan Pro.
5. | Read DTCs.
6. | Find and repair the trouble, and clear the DTCs using Hi-Scan Pro.
7. | Disconnect the Hi-Scan Pro.
DIAGNOSTIC TROUBLESHOOTING FLOW