| TIBURON(GK) >2005 > G 2.0 DOHC > Restraint > Airbag Module > Side Airbag (SAB) Module>Repair procedures |

REMOVAL
1. | Disconnect the battery negative (-) terminal cable.
Wait at least 3 minutes.
2. | Disconnect the side airbag harness 2p connector.
3. | Remove the seat assembly and seat-back cover.
4. | Remove the two mounting nuts and the side airbag.
1. | Never attempt to disassemble or repair the airbag module.
2. | Do not drop the airbag module or allow contact with water, grease or oil. Replace it if a dent, crack, deformation or rust are detected.
3. | The airbag module should be stored on a flat surface and placed so that the pad surface is facing upward. Do not place anything on top of it.
4. | Never attempt to measure the circuit resistance of the airbag module (squib) even if you are using the specified tester. If the circuit resistance is measured with a tester, accidental airbag deployment will result in serious personal injury.