| TIBURON(GK) >2005 > G 2.0 DOHC > Body Electrical System > Horn > Horn>Repair procedures |

REMOVAL
1. | Remove the bolt holding the horn and remove the horn assembly.
2. | Installation is the reverse of removal.
INSPECTION
1. | Test the horn by connecting battery voltage to the 1 terminal and ground the 2 terminal.
2. | The horn should make a sound. If the horn fails to make a sound, replace it.
ADJUSTMENT
After adjustment, apply a small amount of paint around the screw head to keep it from loosening.