| TIBURON(GK) >2005 > G 2.0 DOHC > Engine Mechanical System > Intake And Exhaust System>Repair procedures |

REMOVAL
INTAKE MANIFOLD
1. | Remove the engine cover. (See page EM - 8)
2. | Disconnect the TPS connector(A) and ISA connector(B).
3. | Remove the PCV hose(A) and breather hose(B).
4. | Remove the accelerator cable by loosening the locknut, then slip the cable end out of the throttle linkage.
5. | Remove the delivery pipe(A).
6. | Remove the heater hoses(A), PCSV(B), and brake vacuum hose(C).
7. | Remove the intake manifold stay(A).
8. | Remove the intake manifold.
9. | Installation is in the reverse order of removal.
Exhaust manifold
1. | Remove the engine cover. (See page EM - 8)
2. | Remove the front oxygen sensor connector.
3. | Remove the front muffler(A).
4. | Remove the heat protector.
5. | Remove the exhaust manifold.