| TIBURON(GK) >2005 > G 2.0 DOHC > Body (Interior and Exterior) > Seat & Power Seat > front seat>Repair procedures |

REMOVAL AND INSTALLATION
1. | Pull out front seat mounting cover and remove the bolts.
2. | Remove the front seat assembly.
3. | Remove the seat recliner control lever and seat cushion control knob. Remove the mounting screws from the shield cover.
4. | Remove the front seat back board.
5. | Remove the mounting bolt from the front seat back.
6. | Remove the 4 bolts mounted under the seat to remove the front seat track.
7. | Installation is the reverse of removal.