| TIBURON(GK) >2005 > G 2.0 DOHC > Heating,Ventilation, Air Conditioning > General Information>Specifications |

SPECIFICATIONS
Item | Specification
Heater assembly | Heater Type | Air mix type
Capacity | 4,500 ± 10% kcal/hr
Evaporator | Cooling capacity | 4,100 ± 10% kcal/hr
Compressor | Type | Swash plate (HS-15)
Oil capacity | 140 ~ 160cc
Pressure relief valve | Operating pressure : 35 ~ 42.2kg/cm²
Voltage | D.C 12.8 ± 0.2V
Magnetic clutch | Voltage & wattage | D.C 12.8 ± 0.2V, Max. 54W
Torque | Min. 4.4kg.m
Refrigerant | Capacity | R-134a (600 ± 25g)
Triple pressure switch | High pressure | ON : 32.0 ± 2.0kg/cm² OFF : 26.0 ± 2.0kg/cm²
Middle pressure | ON : 18.0 ± 0.8kg/cm² OFF : 14.0 ± 1.2kg/cm²
Low pressure | ON : 2.3 + 0.25 / -0.29kg/cm² OFF : 2.0 ± 0.2kg/cm²
Thermistor | A/C ON/OFF | ON 3.0 ± 0.6°C OFF : 1.5 ± 0.6°C
Heater control assembly | MANUAL Type, AUTOMATIC Type