| TIBURON(GK) >2005 > G 2.0 DOHC > Body Electrical System > Audio > Audio Remote control>Repair procedures |

REPLACEMENT
1. | Remove the driver airbag module. (Refer to the airbag group)
2. | Remove the audio remote control switch (B) after remove the steering wheel remote control switch connector (A) and 2 screws.
3. | Installation is the reverse of removal.
INSPECTION
1. | Check for resistance between No.1 and No.4 terminals in each switch position.
Switch | Connector terminal | Resistance (±5%)
VOLUME DOWN | 1 - 4 | 6.81 kΩ
VOLUME UP | 1 - 4 | 4.61 kΩ
SEEK UP | 1 - 4 | 430 Ω
POWER ON/OFF | 1 - 4 | 100 Ω