| TIBURON(GK) >2005 > G 2.0 DOHC > Body (Interior and Exterior) > Seat Belt > rear seat belt>Repair procedures |

REPLACEMENT
REAR SEAT BELT REPLACEMENT
1. | After loosening the rear seat back mounting bolt, remove the rear seat back (A).
2. | After loosening the rear seat cushion mounting bolt, remove the rear seat (A).
3. | Remove the trim (A).
4. | Loosening the retractor (A) mounting bolt.
5. | After loosening the lower anchor (B) mounting bolt, remove seat belt (C).
6. | Installation is the reverse of removal.
REAR SEAT BELT BUCKLE REPLACEMENT
1. | Remove the rear seat (See page BD-62).
2. | Remove the seat buckle (A).
3. | Installation is the reverse of removal.