| TIBURON(GK) >2005 > G 2.7 DOHC > Body (Interior and Exterior) > Seat Belt > front seat belt>Repair procedures |

REMOVAL AND INSTAIIATION
1. | Loosen the front seat belt upper anchor mounting bolt.
2. | Loosen the sliding bar mounting bolts.
3. | Loosen the seat belt webbing guide and remove the front seat belt.
4. | Remove the center piller trim and front seat belt height adjuster.
Tightening torque: 39.2~53.9 N•m (4.0~5.5 kgf•m, 28.9~39.8 lbf•ft)
1. | A pretensioner functions one time only. Be sure to replace the pretensioner seat belt after it is deployed.
2. | Do not attempt to disassemble or repair the seat belt pre-tensioner. When it malfunctions, replace with a new pre-tensioner seat belt.
3. | Be cautious in handling a pre-tensioner seat belt, and do not drop it in water, or oil. If crushed, damaged, or deformed, replace it with a newone.
4. | Only connect the battery after installation of the pretensioner seat belt has been correctly completed.
5. | Removal of the pretensioner seat belt :
• | Make sure that ignition is "Off".
• | Disconnect the negative (-) battery terminal and make sure it does not come into contact with the body.
• | Wait for about 1 minute.
• | Pull the plug out from the appropriate connector at the gas generator.
• | Loosen the bolt and remove the belt from the vehicle body.