| TIBURON(GK) >2005 > G 2.7 DOHC > Manual Transaxle System > Manual Transaxle Control System > Manual Transaxle Shift Control>Repair procedures (M5GF1) |

REMOVAL
1. | Remove the shift knob.
2. | Remove the spring and the cap (for 6-speed M/T).
3. | Remove the skirt (for 6-speed M/T).
4. | Remove the console upper cover.
5. | Remove the console assembly.
6. | Remove the shift cable clip.
7. | Remove the select cable clip.
8. | Remove the snap pin of the select cable.
9. | Remove the shift cable.
10. | Remove the shift lever assembly.
For 6-speed M/T, push the plate shaft outward with a driver or equivalent through the hole in the shift lever bracket to remove it.
INSTALLATION
Install the shift lever assembly.
INSPECTION
1. | Check the select cable for proper operation and for damage.
2. | Check the shift cable for proper operation and for damage.
3. | Check the boot for damage.
4. | Check each bushing for wear, abrasion, sticking, restricted movement or damage.
5. | Check for a weak or damaged spring.